# Products checklist

## 🞎 Main headline

JWC Honey Monster

## 🞎 Images

Honey Monster Image

## 🞎 Description

JWC’s Honey Monster® septage receiving station and Fats, Oils and Grease (FOG) receiving system quickly screens and processes septage, grease, FOG or sludge from haul trucks. This automated acceptance plant allows for cleaner handling of septage truck waste by reducing and separating unwanted solids such as rocks and rag. The unique combination of grinding, solids removal, washing and dewatering allows a typical septage truck to unload in 5 to 15 minutes. The septage receiving station is completely enclosed to ensure safety, vector control and containment of foul odours.

The automated Honey Monster septage receiving station makes managing septage waste easy for both the wastewater plant operator and the hauler.  The hauler just connects their cam lock hose and starts the flow.  Septage waste will pass by the **SRS3000 Rock Trap** before the **Muffin Monster grinder** shreds the debris found in septage waste.  Ultrasonic level sensors work with the system’s PLC to modulate the plug valve and regulate the flow into the screening area.  An auger screw and perforated screening trough screens out unwanted debris to protect downstream. Trash is washed, fully compacted and dewatered for disposal with JWC’s unique double helix compaction zone.

The Honey Monster is also available with the optional **Monster Track system.**This option controls hauler access to the septage disposal systems and will provide data for accurate billing.  It provides unique identification of the hauler and tracks the quantity of FOG of septage waste discharged.  The **Monster Track system** can also monitor system levels and can alarm for unexpected pH levels in dumped waste.

## 🞎 Features

* Hauler access control and billing with Monster Track system
* Dual Helix compaction zone for additional dewatering
* High level ultrasonic sensor controls inlet plug valve
* Triple spray wash manifold washes away soft organics
* Optional [Heavy Object Trap (HOT)](https://www.jwce.com/product/rtp/) for pre-screening rocks and metal

## 🞎 Applications

* Handling of septage truck waste
* Handling of FOG waste

## 🞎 Downloads

Honey Monster Brochure

Please add these to the downloads folder.

## 🞎 Video url link

None yet

## 🞎 Tags / categories

I'll use the words tag and category interchangeably.

There are 4 types of categories:

Pump Type, Application, Industry, Brand .

I've put a list here. Just **bold** the ones that this product applies to.

|  |  |  |  |
| --- | --- | --- | --- |
| Pump Type | Application | Industry | Brand |
| Booster set  Bore pumps  Diaphragm pumps  Dosing pumps  Drum pumps  Flexible impeller pumps  Gear Pumps  Macerators  Lobe pumps  Magnetic drive pumps  Mixers  Multistage pumps  Odour filters  Peristaltic hose pumps  Piston pumps  Progressive Cavity Pump  Screw channel pumps  Self priming pumps  Submersible pumps  Twin screw pumps  Eccentric disc pumps | Desalination  Dewatering  Fire  Floodwater  Greywater  Irrigation  **Sewage**  **Sludge**  Stormwater  Water  **Wastewater**  Food & Hygiene | Agriculture  Aquaculture  Building  Environmental  **Industrial**  Mining  **Municipal**  **Wastewater** | Abaque  Caprari  Cornell  Ebara  Flygt  Gorman-Rupp  Grundfos  Hidrostal  Inoxpa  **JWC**  KSB  Lowara  Mono  Netzsch  Paco  Remko  Roto  Southern Cross  Spel  Sulzer  Tsurami  Verderflex  Waterco  Wilden  Zenit  Zenox |

When we add products in the website administration area, we can categorise them using the list you provide above.